|  |  |
| --- | --- |
| Product name and model | Auto focus motor with medium and high pixel camera |
| Main technical performance indexof the product | Function: Auto FocusSuitable pixel: 8M/13M/16M |
| Compared with the old products, what are the improvements(structure,material, technology,process,performance, use function) |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Old products | New product | utility |
| structure | Metal shell | The metal case is provided with a plastic outer cover | Flexibly match the motor height |
| Design Technique | The spring plate is arranged inside the metal shell | The spring plate is arranged outside the metal shell | Provide ample design space for shrapnel |
| Technology | Traditional craft | The plastic outer cover is riveted with the metal shell | The plastic outer cover providesthe required joint area of the cushion |
| Performance | Dynamic axis tilt angle: less than 0.25 (15 points) | Dynamic axis tilt angle: less than 0.167 (10 points) | Adaptation to high pixel image quality requirements。 |
| Use function |  General specifications AF. | Auto focus, long stroke. | Applicable to high pixel lens range image. |

With the mobile phone, the new product, the high pixel camera autofocus motor, has the following improvements: |